;------------------------------------------------------------------------
; btnulmdm.inf
; IVT Corporation Bluetooth NULL Modem Installation Script
; For Windows98SE/ME/2000/XP
;
; Copyright (c) 2000-2004, IVT Corporation.
; http://www.ivtcorporation.com
; http://www.bluesoleil.com
;
;------------------------------------------------------------------------

[Version]
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Provider%
DriverVer=12/6/2004,1.2.1
CatalogFile=btnulmdm.cat

[Manufacturer]
%IVT% = IVT

[IVT]
%STDBTNUL% = STDBTNUL, {F12D3CF8-B11D-457e-8641-BE2AF2D6D204}\MDMBTNULL

[STDBTNUL]
AddReg=All, STDBTNULReg, 115200, SERIAL

[All]
HKR,,FriendlyDriver,,Unimodem.vxd
HKR,,DevLoader,,*VCOMM
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"

; DeviceTypes
[SERIAL]
;Install not as a NULL Modem
HKR,, DeviceType, 1, 01


; DCB's - dwords and words are byte reversed
;                                                                           ByteSize (Number of bits/byte, 4-8)
;                                                                               Parity (0-4=None,Odd,Even,Mark,Space)
;                                                                                   StopBits (0,1,2 = 1, 1.5, 2)
;              |DCBLength   |BaudRate    |Bit Mask    |Rsvd  |XonLim|XofLim|   |   |   |Xon|Xof|Err|Eof|Evt
[115200]
HKR,, DCB, 1, 1C,00,00,00, 00,C2,01,00, 15,20,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00

[STDBTNULReg] ; Null-Modem
HKR, Init, 1,, "None"
HKR, Init, 2,, "NoResponse"
HKR, Monitor, 1,, "None"
HKR, Answer, 1,, "CLIENTSERVER"
HKR, Answer, 2,, "NoResponse"
HKR, Settings, DialPrefix,, "CLIENT"
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 30,00,00,00, 00,c2,01,00, 00,c2,01,00
HKR, Responses, "CLIENT",       1, 08, 00, 00, 00, 00, 00, 00,00,00,00 ; Server side - the client is requesting a connection
HKR, Responses, "<h00>CLIENT",  1, 08, 00, 00, 00, 00, 00, 00,00,00,00 ; Server side - the client is requesting a connection
HKR, Responses, "CLIENTSERVER", 1, 02, 00, 00, 00, 00, 00, 00,00,00,00 ; Client side - the server has acknowledged and the connection is completed
HKR, Clients\Ras, EnableForRas, 0x00010001, 1


[Strings]
Provider = "IVT Corporation"
IVT = "IVT Corporation"
STDBTNUL = "Bluetooth LAP Modem"
