;; netrtwlanu.inf 
;;
;; NETGEAR A7000 WiFi Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Netgear%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 12/25/2017,1030.25.0701.2017



[Manufacturer]
%Netgear% = Netgear,NTamd64.10.0

[ControlFlags]
ExcludeFromSelect = *

[Netgear.NTamd64.10.0]

;;----------------------------------------------------------------------------
;; For 8814A Netgear
;;----------------------------------------------------------------------------
%Netgear-A7000.DeviceDesc% 				= RTL8814au.ndi, 	USB\VID_0BDA&PID_8813
%Netgear-A7000.DeviceDesc% 				= RTL8814au.ndi, 	USB\VID_0846&PID_9054

;;----------------------------------------------------------------------------
;; Realtek 8814AU default installation
;;----------------------------------------------------------------------------
[RTL8814au.ndi.NT]
AddReg				= NDIS_64.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, RTL8814au.common.reg, KFREE_COMMON.reg, VHT24G.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8814au.ndi.NT.Services]
AddService			= A7000, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8814au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles
;;
;; OS relative registry.
;;
[NDIS_64.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan,ethernet,vwifi"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %Netgear-A7000.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\A7000.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

[MCCDisable.reg]
HKR,Ndi\params\MultiChannelFcsMode, 		ParamDesc, 	0, "Multi-Channel Concurrent"
HKR,Ndi\params\MultiChannelFcsMode, 		type, 		0, "enum"
HKR,Ndi\params\MultiChannelFcsMode, 		default, 	0, "0"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"0", 		0, "Disabled"
HKR,Ndi\params\MultiChannelFcsMode\enum, 	"12", 		0, "Enabled"
HKR,defaults,MultiChannelFcsMode, 0, "0"
HKR,,MultiChannelFcsMode, 0, "0"

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
;HKR,,SSPwrLvl,0,"2"


;; For Different AC mode Rx parameters.
HKR,,AcUsbDmaTime,0,"10"
HKR,,AcUsbDmaSize,0,"5"
HKR,,AcUsbDmaTime2,0,"32"
HKR,,AcUsbDmaSize2,0,"5"


;; For Init mode
HKR,,FWOffload,0,"2"


;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;; For Hotspot UI Select Network Band
HKR,defaults,WdiGOon5GHzBandSupported,0,"0"
HKR,,WdiGOon5GHzBandSupported,0,"0"

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"


;-------------------------------------------------------------------------------
;     Timer GPIO.
;-------------------------------------------------------------------------------
[TimerGPIOSetting8812AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"1"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;-------------------------------------------------------------------------------
;	Custom Tx Power Limit And Power By Rate Parameters
;-------------------------------------------------------------------------------
[CustomTxPwrConfigFile.reg]
HKR,,PwrByRateFile,0,"A7000.txt"
HKR,,PwrLimitFile,0,"A7000_LMT.txt"

;*******************************************************************************
; RTL8814au common paramters
;*******************************************************************************
[RTL8814au.common.reg]
HKR,,UsbRxAggMode,0,"1"
HKR,,IQKFWOffload,0,"0"
HKR,,UsbTxAggTotalNum,0,"24"
HKR,,UsbTxAggDescNum,0,"3"

HKR,,FWOffload,0,"2"
HKR,,ValidRFPath,0,"495"
HKR,,PreInitMem,0,"1"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"
HKR,,RxReorder_FlushChk,0,"1"

;; Enable AMSDU of AMPDU.
HKR,Ndi\params\AMfactor,        ParamDesc,  0, "AMfactor"
HKR,Ndi\params\AMfactor,        type,       0, "enum"
HKR,Ndi\params\AMfactor,        default,    0, "7"
HKR,Ndi\params\AMfactor\enum,   "7",        0, "VHT AMPDU"
HKR,Ndi\params\AMfactor\enum,   "252",      0, "VHT AMSDU in AMPDU Mode 1"
HKR,Ndi\params\AMfactor\enum,   "253",      0, "VHT AMSDU in AMPDU Mode 2"
;;HKR,Ndi\params\AMfactor\enum,   "254",        0, "VHT LDPC TX"
HKR,Ndi\params\AMfactor\enum,   "251",      0, "VHT AMSDU in AMPDU Mode Manual"
HKR,defaults,AMfactor,0,"253"
HKR,,AMfactor,0,"253"
HKR,,AMfactor,,"253"

;; STBC 
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "17",        0, "HT/VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "34",        0, "HT/VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; LDPC 
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "17",        0, "HT/VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "34",        0, "HT/VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;; BEAMFORMING
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "0"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "17",        0, "HT/VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "34",        0, "HT/VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"51"
HKR,,BeamformCap,0,"51"
HKR,,BeamformCap,,"51"

;; USB Switch Fast Mode
HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "1"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"1"
HKR,,UsbSwFast,0,"1"

;; USB Device/Host Control RF Path
HKR,Ndi\params\UsbRfSet, 	ParamDesc, 	0, "USB RF SELECT"
HKR,Ndi\params\UsbRfSet, 	type, 		0, "enum"
HKR,Ndi\params\UsbRfSet, 	default, 	0, "0"
HKR,Ndi\params\UsbRfSet\enum, 	"0", 	0, "BY DEV/HOST"
HKR,Ndi\params\UsbRfSet\enum, 	"1", 	0, "HW DEFAULT SET"
HKR,defaults,UsbRfSet,0,"0"
HKR,,UsbRfSet,0,"0"


;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,bNewRcvRefCnt,0,"1"
HKR,,bNewRcvRefCnt,0,"1"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

HKR,,PreferBand,0,"2"

;;Tx power limit
HKR,,EnableTxPowerLimit,0,"2"

;; For QoS test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\QoS,        ParamDesc,  0, "QoS Support"
HKR,Ndi\params\QoS,        type,       0, "enum"
HKR,Ndi\params\QoS,        default,    0, "0"
HKR,Ndi\params\QoS\enum,   "0",        0, "Not Support QoS"
HKR,Ndi\params\QoS\enum,   "1",        0, "Support QoS"
HKR,Ndi\params\QoS\enum,   "2",        0, "Auto"
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,,QoS,,"1"


HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"
HKR,defaults,RegRxReorder_WinSize,0,"128"
HKR,,RegRxReorder_WinSize,0,"128"
HKR,defaults,RxReorder_PendTime,0,"100"
HKR,,RxReorder_PendTime,0,"100"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"0"

HKR,defaults,AddbaReqRetry,0,"0"
HKR,,AddbaReqRetry,0,"0"

;;Define enable status of each RT Bug Check IDs
HKR,,BugCheckIdLogEnConfig,0x10001,0x7FFF


;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

HKR,defaults,PHYParaFromFolder,0,"0"
HKR,,PHYParaFromFolder,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

HKR,Ndi\params\EnableAdaptivity, 		ParamDesc, 	0, "EnableAdaptivity"
HKR,Ndi\params\EnableAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\EnableAdaptivity, 		default, 	0, "0"
HKR,Ndi\params\EnableAdaptivity\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"1", 		0, "Enable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"2", 		0, "Auto"
HKR,defaults,EnableAdaptivity, 0, "2"
HKR,,EnableAdaptivity, 0, "2"

HKR,Ndi\params\L2HForAdaptivity, 		ParamDesc, 	0, "L2HForAdaptivity"
HKR,Ndi\params\L2HForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\L2HForAdaptivity, 		default, 	0, "Auto"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"0", 		0, "Auto"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"245", 		0, "F5"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"243", 		0, "F3"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"241", 		0, "F1"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"239", 		0, "EF"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"237", 		0, "ED"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"235", 		0, "EB"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"232", 		0, "E8"
HKR,defaults,L2HForAdaptivity, 0, "0"
HKR,,L2HForAdaptivity, 0, "0"

HKR,Ndi\params\HLDiffForAdaptivity, 		ParamDesc, 	0, "HLDiffForAdaptivity"
HKR,Ndi\params\HLDiffForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\HLDiffForAdaptivity, 		default, 	0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"7", 		0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"9", 		0, "9"
HKR,defaults,HLDiffForAdaptivity, 0, "7"
HKR,,HLDiffForAdaptivity, 0, "7"

HKR,Ndi\params\AdaptivityPara, 		ParamDesc, 	0, "AdaptivityPara"
HKR,Ndi\params\AdaptivityPara, 		type, 		0, "enum"
HKR,Ndi\params\AdaptivityPara, 		default, 	0, "0"
HKR,Ndi\params\AdaptivityPara\enum, 	"0", 		0, "0"
HKR,Ndi\params\AdaptivityPara\enum, 	"1", 		0, "1"
HKR,defaults,AdaptivityPara, 0, "0"
HKR,,AdaptivityPara, 0, "0"

; TPC mechenisum
; HKR,Ndi\params\TPCEnable,        ParamDesc,  0, "TPCEnable"
; HKR,Ndi\params\TPCEnable,        type,       0, "enum"
; HKR,Ndi\params\TPCEnable,        default,    0, "0"
; HKR,Ndi\params\TPCEnable\enum,   "0",        0, "TPC Disable"
; HKR,Ndi\params\TPCEnable\enum,   "1",        0, "ETSI Enable"
; HKR,Ndi\params\TPCEnable\enum,   "2",        0, "MKK Enable"
; HKR,Ndi\params\TPCEnable\enum,   "4",        0, "FCC Enable"
; HKR,Ndi\params\TPCEnable\enum,   "8",        0, "WW Enable"
; HKR,Ndi\params\TPCEnable\enum,   "15",        0, "Enable All"
; HKR,defaults,TPCEnable,0,"0"
; HKR,,TPCEnable,0,"0"

; HKR,Ndi\params\TxPowerControl,        ParamDesc,  0, "TxPowerControl"
; HKR,Ndi\params\TxPowerControl,        type,       0, "enum"
; HKR,Ndi\params\TxPowerControl,        default,    0, "0"
; HKR,Ndi\params\TxPowerControl\enum,   "0",        0, "100%"
; HKR,Ndi\params\TxPowerControl\enum,   "1",        0, "50%"
; HKR,Ndi\params\TxPowerControl\enum,   "2",        0, "0"
; HKR,defaults,TxPowerControl,0,"0"
; HKR,,TxPowerControl,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

[N61RxReorder.reg]
HKR,defaults,RegRxReorder_WinSize,0,"64"
HKR,,RegRxReorder_WinSize,0,"64"
HKR,defaults,RxReorder_PendTime,0,"30"
HKR,,RxReorder_PendTime,0,"30"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%%SystemRoot%%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,Ndi\params\WirelessMode\enum, 	"256", 		0, %IEEE_802_11AC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"10"
HKR,,RFType,0,"15"

HKR,,BWSetting,0,"2"


;;----------------------------------------------------------------------------
;; 11AC series IC VHT 2.4G Support
;;----------------------------------------------------------------------------
[VHT24G.reg]
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "255"
HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"255", 		0, "Enable"
HKR,Ndi\params\Vht24g\enum, 	"254", 		0, "Not support Broadcom vendor"
HKR,defaults,Vht24g, 0, "255"
HKR,,Vht24g, 0, "255"

;;----------------------------------------------------------------------------
;; KFree parameters
;;----------------------------------------------------------------------------
[KFREE_COMMON.reg]
HKR,,RfKFreeEnable,0,"0"


;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
A7000.sys, rtwlanu.sys,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12
CoInstaller.CopyFiles = 11

;;****************************************************************************
;; Source Files
;;****************************************************************************

[SourceDisksFiles]
rtwlanu.sys = 1
rtlCoInst.dll = 1
rtlCoInst.dat = 1

[SourceDisksNames]
1=%DISKNAME%,,,
[CoInstaller.AddReg]
HKR,,CoInstallers32,0x10000,"rtlCoInst.DLL,rtlCoInst"

[CoInstaller.CopyFiles]
rtlCoInst.dll,,,0x04
rtlCoInst.dat,,,0x04
;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
WL_MODE_STR					= "Wireless Mode"
AUTO_STR 				    = "Auto"
IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
IEEE_802_11AC_STR			= "IEEE 802.11 ac"


;*******************************************************************************
; manufacture description
;*******************************************************************************
Netgear					= "NETGEAR Inc."

;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
Netgear-A7000.DeviceDesc 				= "NETGEAR A7000 WiFi USB3.0 Adapter"
Netgear-A7000.DeviceDesc.DispName		= "NETGEAR A7000 WiFi USB3.0 Adapter"
