;------------------------------------------------------------------------
;
;   IR decoder driver Install Information File
;
;       V1.0.1.8 2005/12/06 00:00:00
;
;   Copyright (c) 2005 DTV-DVB Technology Inc.
;   All Rights Reserved.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"

Class=HIDClass
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}

Provider="DTV-DVB"
DriverVer=12/06/2005,1.0.1.8
CatalogFile.ntx86=3054IR.cat

[Manufacturer]
"DTV-DVB"=DTV-DVB

[SourceDisksNames]
1="DTV-DVB PCI Drivers",,,""

[SourceDisksFiles]
3054IR.sys=1

[DTV-DVB]
;FMD1216 + MT352
%THDVBT.DeviceDesc%=THDVBT,                     PCI\VEN_14F1&DEV_8804&SUBSYS_00191822
%THDVBT.DeviceDesc%=THDVBT,                     PCI\VEN_14F1&DEV_8804&SUBSYS_00251822

[THDVBT]
Include=    ks.inf
Needs=      KS.Registration
AddReg=     THIR.AddReg,THDVBT.AddReg
CopyFiles=  THIR.CopyDrivers

[DestinationDirs]
THIR.CopyDrivers=10,system32\drivers

[THIR.CopyDrivers]
3054IR.sys

[THIR.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,3054IR.sys

;
; Driver Configuration Registry Entries
;

[THDVBT.AddReg]
;NEC standard
HKR,"DriverData","IR_Standard",0x00010001, 0x01, 0x00, 0x00, 0x00
;command table
; 0: DTV-DVB remote, 1: CyberLink, 2: IVI, 3: MCE, 4: DTV-DVB (WM_INPUT), 5: Custom, 0xFFFF: Disable RC
HKR,"DriverData","RC_Configuration",0x00010001, 0x00, 0x00, 0x00, 0x00

;Configurable RC Hot keys
;HKR,"DriverData","RC_Configuration",0x00010001, 0x05, 0x00, 0x00, 0x00
 
; Scan code mappings.
; Format: SCANCODE_nn = 0xii, 0xjj, 0xkk, 0xll
;   nn: hex value of scan code (Please reference DTV-DVB RC table)
;   ii: first virtual key value
;   jj: ctrl virtual key value
;   kk: shift virtual key value
;   ll: alt virtual key value
; Note: 1) Refer to MSDN for virtual key values (keyword: "VK_")
;       2) Maximum three key combination supported now
;
;HKR,"DriverData","RC_Scancode_00",0x00010001, 0x09,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_01",0x00010001, 0x09,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_02",0x00010001, 0x09,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_03",0x00010001, 0x09,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_04",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_05",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_06",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_07",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_08",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_09",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_0A",0x00010001, 0x00,0x00, 0x00, 0x00

;.....
;.....
;HKR,"DriverData","RC_Scancode_71",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_72",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_73",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_74",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_75",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_76",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_77",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_78",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7A",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7B",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7C",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7D",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7E",0x00010001, 0x00,0x00, 0x00, 0x00
;HKR,"DriverData","RC_Scancode_7F",0x00010001, 0x00,0x00, 0x00, 0x00

HKR,"DriverData","RC_Scancode_15",0x00010001, 0x30,0x00, 0x00, 0x00
HKR,"DriverData","RC_Scancode_03",0x00010001, 0x31,0x00, 0x00, 0x00
HKR,"DriverData","RC_Scancode_01",0x00010001, 0x32,0x00, 0x00, 0x00
HKR,"DriverData","RC_Scancode_06",0x00010001, 0x33,0x00, 0x00, 0x00
HKR,"DriverData","RC_Scancode_09",0x00010001, 0x34,0x00, 0x00, 0x00


;This is the IR system code (2 bytes) for INF file registry key.
; //IR system code checklist1 (00,FF)
HKR,"DriverData","IRSYSCODECHECK1",0x00010001, 0x00,0xFF,0x00,0x00
; //IR system code checklist2 (01,AA)
;HKR,"DriverData","IRSYSCODECHECK2",0x00010001, 0x01,0xAA,0x00,0x00

;
; Services installation
;

;
;  DTV-DVB DVB-T, FMT1216 + MT352
;
[THDVBT.Services]
AddService = THIR,2,THDVBT.ServiceInstall

[THDVBT.ServiceInstall]
DisplayName   = %THDVBT.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\3054IR.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
THDVBT.DeviceDesc               = "DTV-DVB 3054 IR Decoder"

