; Cmd191c1p.inf
; Setup information file for MITSUBISHI LCD Monitor MD191C1P
;
; Copyright (C) 2005 Mitsubishi Electric Corporation
;---------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%MITSUBISHI%
CatalogFile=md191c1p.cat
DriverVer=04/07/2005,1.05.0407.1703

[ControlFlags]
ExcludeFromSelect.nt=Monitor\MEL4712
ExcludeFromSelect.nt=Monitor\MEL4713

[DestinationDirs]
MD191C1P.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
md191c1p.icm=1

[Manufacturer]
%MITSUBISHI%=MITSUBISHI

[MITSUBISHI]
%MD191C1P-A%=MD191C1P-A.Install, Monitor\MEL4712
%MD191C1P-D%=MD191C1P-D.Install, Monitor\MEL4713

[MD191C1P-A.Install]
DelReg=DEL_CURRENT_REG
AddReg=MD191C1P-A.AddReg, 1280, DPMS
CopyFiles=MD191C1P.CopyFiles

[MD191C1P-D.Install]
DelReg=DEL_CURRENT_REG
AddReg=MD191C1P-D.AddReg, 1280, DPMS
CopyFiles=MD191C1P.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[MD191C1P-A.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-82.0,48.0-85.0,+,+"
HKR,,ICMProfile,0,"md191c1p.icm"

[MD191C1P-D.AddReg]
HKR,"MODES\1280,1024",Mode1,,"31.0-82.0,48.0-85.0,+,+"
HKR,,ICMProfile,0,"md191c1p.icm"

[MD191C1P.CopyFiles]
md191c1p.icm

[Strings]
MITSUBISHI="MITSUBISHI"
MD191C1P-A="MITSUBISHI TFT MD191C1P (Analog)"
MD191C1P-D="MITSUBISHI TFT MD191C1P (Digital)"
Disk1="Mitsubishi Display Monitor Installation Disk"
